<?xml version="1.0" encoding="UTF-8"?>

<section xml:id="introCodeplug" 
         xmlns="http://docbook.org/ns/docbook" 
         xmlns:xlink="http://www.w3.org/1999/xlink" 
         xmlns:xi="http://www.w3.org/2001/XInclude">

<info>
  <title>Codeplug Assembly</title>
</info>

<para>
  After the basic concepts and technical details of the DMR mode has been discussed, it is time to 
  consider the actual configuration of the DMR radios. This usually not done via the keypad of the 
  radio but with the help of a separate software. The so-called <glossterm>CPS</glossterm> or 
  codeplug programming software. 
</para>

<para>
  Before we can start, we need like any other participant in the DMR network a unique number, the 
  DMR ID.
</para>

<note>
  <para>
    You can get your personal and unique DMR ID from 
    <link xlink:href="https://www.radioid.net/">radioid.net</link>. There you need to verify that
    you are a licensed ham operator.
  </para>
</note>

<para>
  You will receive your personal DMR ID usually within 24h per Mail. Once you've got your ID, 
  you can start.
</para>

<para>
  As this script is intended for the beginners, it is very likely that you do not own a top-shelf 
  Motorola device but rather one of the cheap devices of the common manufacturers.
</para>

<warning>
  <para>
    If you do not own a DMR device yet but consider to by one, you should explicitly check whether 
    it supports DMR Tier I and II<footnote><para>As usual, DMR is not a single standard but a 
      family of standards. Tier I describes the simplex operation while Tier II considers the 
      repeater operation and time-slots. You will therefore need a device that also implements 
      Tier II to be able to work with repeaters.</para></footnote>. Ignore any marketing BS and
      check the technical description of the product for Tier I &amp; II. If it is not mentioned
      there, simply skip that product. This is particularly true for the Baofeng MD-5R but not 
      the RD-5R. 
  </para>
</warning>

<para>
  The manufacturer of the device of your choice will provide the CPS for download you need to program
  your radio. Usually you will also find there firmware updates for your device. The manufacturers 
  usually provide a separate CPS version for every device and even firmware revision. So please check
  whether you've got the correct CPS version. The configuration of the device differs from device to
  device and even more from manufacturer to manufacturer. The basic setup, however, remains the same.
</para>

<para>
  When you start the CPS for the first time, you will likely note two things. First, that the user 
  experience stems from the last millennium (about Windows 3.11). And second, that there are a tone
  of obscure and badly translated options for your device. These options are usually named cryptic
  and are not documented. 
</para>

<para>
  The configuration of your device usually happens in five to six steps:
</para>
<orderedlist>
  <listitem><para>General settings, </para></listitem>
  <listitem><para>creating contacts, </para></listitem>
  <listitem><para>assembling group lists, </para></listitem>
  <listitem><para>creating channels, </para></listitem>
  <listitem><para>assembling zones and </para></listitem>
  <listitem><para>optionally assembling scan lists.</para></listitem>
</orderedlist>

<para>
  Within the following sections, I want to guide you through these steps.
</para>


<section xml:id="introCPGeneral">
<info><title>General radio-wide settings.</title></info>

<para>
  The single most important options within the general settings is your DMR ID and your call sign. These 
  options are usually located under the label <guilabel>Radio Settings</guilabel> or 
  <guilabel>General Settings</guilabel><footnote><para>The actual name may vary from manufacturer
    to manufacturer.</para></footnote>.
  Your DMR ID is entered in the field name <guilabel>Radio ID</guilabel>. Many radios support to 
  enter several DMR IDs. This feature is usually not used in ham radio. In fact you will only always
  need a single DMR ID even with several radios.
</para>

<para>
  Your call can be entered in the <guilabel>Radio Name</guilabel> field.
</para>
</section>


<section xml:id="introCPContact">
<info><title>Creating Contacts</title></info>

<para>
  Once you have made these basic settings, you may create some contacts in your contact list. This 
  list should contain all talk groups you are interested in, some private contacts to OM you know
  as well as some <quote>service numbers</quote> for the <quote>echo</quote>-service, SMS service 
  etc. A sample is shown in <xref linkend="tabIntroContacts"/>.
</para>

<table xml:id="tabIntroContacts">
  <title>Example contacts for germany</title>
  <thead>
    <tr><td>Name</td> <td>Typ</td> <td>Nummer</td>  <td>Name</td> <td>Typ</td> <td>Nummer</td></tr>
  </thead>
  <tbody>
    <tr><td>Local</td>       <td>group call</td> <td>9</td>     <td>Ham/SlHo</td>  <td>group call</td> <td>2622</td></tr>
    <tr><td>Regional</td>    <td>group call</td> <td>8</td>     <td>NiSa/Bre</td>  <td>group call</td> <td>2623</td></tr>
    <tr><td>TG99</td>        <td>group call</td> <td>99</td>    <td>NRW</td>       <td>group call</td> <td>2624</td></tr>
    <tr><td>All call</td>    <td>all call</td> <td>16777215</td> <td>RhPf/Saar</td> <td>group call</td> <td>2625</td></tr>
    <tr><td>World wide</td>  <td>group call</td> <td>91</td>    <td>Hessen</td>    <td>group call</td> <td>2626</td></tr>
    <tr><td>Europe</td>      <td>group call</td> <td>92</td>    <td>BaWü</td>      <td>group call</td> <td>2627</td></tr>
    <tr><td>D-A-CH</td>      <td>group call</td> <td>920</td>   <td>Bay</td>       <td>group call</td> <td>2628</td></tr>
    <tr><td>Germany</td>     <td>group call</td> <td>262</td>   <td>Sa/Th</td>     <td>group call</td> <td>629</td></tr>
    <tr><td>Austria</td>     <td>group call</td> <td>232</td>   <td>Echo Test</td> <td>private call</td> <td>262997</td></tr>
    <tr><td>Switzerland</td> <td>group call</td> <td>228</td>   <td>SMS Serv.</td> <td>private call</td> <td>262993</td></tr>
    <tr><td>EMCOM EU</td>    <td>group call</td> <td>9112</td>  <td>DAPNET</td>    <td>private call</td> <td>262994</td></tr>
    <tr><td>EMCOM WW</td>    <td>group call</td> <td>9911</td>  <td>APRS GW</td>   <td>private call</td> <td>262999</td></tr>
    <tr><td>MeVo/SaAn</td>   <td>group call</td> <td>2620</td>  <td>DM3MAT</td>    <td>private call</td> <td>2621370</td></tr>
    <tr><td>Ber/Bra</td>     <td>group call</td> <td>2621</td>  <td>...</td>       <td>...</td>          <td>...</td></tr>
  </tbody>
</table>

<para>
  Of cause there are much more talk groups. There are also talk groups for specific topics which 
  are not necessarily targeted at a specific region. A rather complete list can be found in the 
  <link xlink:href="https://wiki.brandmeister.network/index.php/TalkGroups">Brandmeister Wiki</link>.
</para>
</section>


<section xml:id="introCPGroupList">
<info><title>Assemble group lists</title></info>

<para>
  The next step is to assemble so-called <glossterm>Group List</glossterm>s. These are simple lists of 
  talk groups that you want to receive on a particular channel. As mentioned in the introduction, the 
  network does not know which talk groups you are interested in. This must be programmed into the radio.
  Group lists do exactly that: The specify which talk groups you want to receive. All others are ignored.
</para>

<para>
  You should at least create two group lists. One for the simplex operation, one for regional communication
  and optionally one for the trans-regional communication. You should also create one for each region you 
  frequently visit.
</para>

<para>
  The simplex group list is theoretically not necessary as simplex calls should always use the so-called 
  <glossterm>All Call</glossterm>. Frequently, however, also the talkgroups TG99, TG9 and TG8 are used 
  in simplex operation. Hence a group list with these talk groups is needed for simplex operation.
</para>

<para>
  Your trans-regional talk group should include the talk groups for the entire world TG91, your 
  continent (e.g., Europe TG92), your country (e.g., Germany TG262) and also the emergency talk 
  group (e.g., 9112 in Europe).
</para>

<para>
  Finally the talk group for the local/regional communication should contain the local TG9, 
  regional TG8 and the talk group for your region (e.g., TG 2621 for my region Berlin/Brandenbug).
  As I am also frequently in saxony, I also created a group list for that region. My 
  group list settings are shown in <xref linkend="tabIntroGroupLists"/>.
</para>
  
<table xml:id="tabIntroGroupLists">
  <title>Example group lists</title>
  <thead>
    <tr><td>Name</td> <td>Group calls</td></tr>
  </thead>
  <tbody>
    <tr><td>Simplex</td> <td>Local, Regional, TG99</td></tr>
    <tr><td>WW/EU/DL</td> <td>World wide, Europe, D-A-CH, Germany, EMCOM EU</td></tr>
    <tr><td>Ber/Bra</td> <td>Local, Regional, Ber/Bra</td></tr>
    <tr><td>Sa/Th</td> <td>Local, Regional, Sa/Th</td></tr>
  </tbody>
</table>
</section>


<section xml:id="introCPChannel">
<info><title>Creating channels</title></info>

<para>
  Before we start assembling any channels, I should mention that DMR radios are also able to 
  transmit and receive analog FM. Thus, you can also use them for classic FM simplex and repeater 
  operation. In this section, I describe the configuration of digital DMR channels usually called 
  <quote>digital channels</quote>. The configuration of analog FM channels is not described. To 
  create a DMR channel, you have to select <guilabel>digital</guilabel> for the <guilabel>channel 
  type</guilabel>, for FM channels <guilabel>analog</guilabel>.
</para>

<para>
  When you already have some experience with the analog FM repeater operation, the configuration 
  of DMR channels may appear quiet weird. For analog FM repeaters, you usually configure exactly 
  one channel. For DMR repeaters you will configure at least two (one for each time slot), but 
  usually many more. To cut a long story short, let me explain it with a concrete example.
</para>


<section>
<info><title>Creating Simplex Channels</title></info>
<table xml:id="tabIntroCPSimplexChannels">
  <title>Example simplex channel configuration</title>
  <thead>
    <tr><td>Name</td> <td>RX Freq.</td> <td>TX Freq.</td> <td>TS</td> <td>CC</td> <td>TX Contact</td> <td>Grp.List</td></tr>
  </thead>
  <tbody>
    <tr><td>DMR S0</td> <td>433.4500 MHz</td> <td>433.4500 MHz</td> <td>1</td> <td>1</td> <td>all call</td> <td>simplex</td></tr>
    <tr><td>DMR S1</td> <td>433.6125 MHz</td> <td>433.6125 MHz</td> <td>1</td> <td>1</td> <td>all call</td> <td>simplex</td></tr>
    <tr><td>...</td> <td>...</td> <td>...</td> <td>...</td> <td>...</td> <td>...</td> <td>...</td></tr>
  </tbody>
</table>

<para>
  In <xref linkend="tabIntroCPSimplexChannels"/> an example for a simplex channel configuration is 
  shown. Of cause, you should extend it to all 8 simplex channels. The first column simply specifies
  the name of the channel.
</para>

<para>
  The second and third columns specify the transmit and receive frequencies for these channels.
  For simplex channels, RX and TX frequencies are the same.
</para>  

<para>
  In simplex operation, there is no repeater. That is, no instance that dictates a beat. To this 
  end the choice of the time slot (TS) is irrelevant and usually TS1 is chosen.
</para>

<para>
  The color code, however, matters. Repeater as well as your radio will ignore calls with a mismatching
  color code. For simplex channels, the color code 1 has been established.
</para>

<para>
  The sixth column specifies the default transmit contact. For simplex channels, the so-called 
  <glossterm>All Call</glossterm> should be chosen, to ensure that really everyone can receive the 
  call irrespective of the receivers group list settings. The default transmit contact specifies 
  the contact (private, group or all call) that is called whenever the PTT is pressed. As mentioned
  earlier, there is an exception to that rule. Whenever you directly answer a call within in the 
  so-called <glossterm>Hang Time</glossterm>, you will answer with the same call you received. 
</para>

<para>
  The last column specifies the to so-called <glossterm>Group List</glossterm>. This list specifies
  which talk groups are received on that channel. As mentioned earlier, no entry should be needed 
  here, as the all-call should be used for the transmit contact on simplex channels. Unfortunately,
  it is not uncommon to find several talk groups being used as transmit contacts on simplex 
  channels like TG9, TG8, TG99. For these cases, a group list <quote>simplex</quote> was created 
  earlier.
</para>

<para>
  Within your CPS, you will find many more options for channels. The majority can be left 
  untouched. At the end of this section, I will describe some of these settings briefly. Many of 
  these settings are quite uncommon in amateur radio or even straight illegal.
</para>

<para>
  The <glossterm>Admit Criterion</glossterm> specifies under which conditions your radio is 
  allowed to transmit. For simplex channels, the option <guilabel>channel free</guilabel> should be
  chosen. This configures the radio to only transmit if the channel is currently free.
</para>
</section>

<section>
<info><title>Creating repeater channels</title></info>

<para>
  Creating repeater channels is slightly more complex than creating simplex channels, as we need to
  create several channels per repeater. Before you can create any channels, you need to know which 
  DMR repeaters are near to you. A good overview provides the
  <link xlink:href="https://repeaterbook.com">repater book</link>. There you can also filter for
  DMR repeaters and you get all information you need to configure the DMR repater channels. That 
  is input and output frequencies and the color code of the repeater.
</para>

<table orient="land" xml:id="tabIntroCPRepeaterChannels">
  <title>Example channels for a single repeater DB0LDS</title>
  <thead>
    <tr><td>Name</td> <td>RX Freq. (output)</td> <td>TX Freq. (input)</td> <td>TS</td> <td>CC</td> <td>TX Contact</td> <td>Grp.List</td></tr>
  </thead>
  <tbody>
    <tr><td>DB0LDS TS1</td> <td>439.5625 MHz</td> <td>431.9625 MHz</td> <td>1</td> <td>1</td> <td>-</td> <td>WW/EU/DL</td></tr>
    <tr><td>DB0LDS DL TS1</td> <td>439.5625 MHz</td> <td>431.9625 MHz</td> <td>1</td> <td>1</td> <td>Germany</td> <td>WW/EU/DL</td></tr>
    <tr><td>DB0LDS Sa/Th TS1</td> <td>439.5625 MHz</td> <td>431.9625 MHz</td> <td>1</td> <td>1</td> <td>Sa/Th</td> <td>Sa/Th</td></tr>
    <tr><td>DB0LDS TG9 TS2</td> <td>439.5625 MHz</td> <td>431.9625 MHz</td> <td>2</td> <td>1</td> <td>TG9</td> <td>Ber/Bra</td></tr>
    <tr><td>DB0LDS TG8 TS2</td> <td>439.5625 MHz</td> <td>431.9625 MHz</td> <td>2</td> <td>1</td> <td>TG8</td> <td>Ber/Bra</td></tr>
    <tr><td>DB0LDS BB TS2</td> <td>439.5625 MHz</td> <td>431.9625 MHz</td> <td>2</td> <td>1</td> <td>Ber/Bra</td> <td>Ber/Bra</td></tr>
  </tbody>
</table>

<para>
  I think, it is the best to explain the creation of repeater channels using a concrete example for
  a repeater near to me shown in <xref linkend="tabIntroCPRepeaterChannels"/>. This repeater has 
  the call DB0LDS and has the input frequency 431.9625 MHz and output frequency 439.5625 MHz. 
  According to repeater book, this repeater expects the color code 1. These are the elementary 
  information you need to set for all channels using this repeater. Many CPSs allow to copy or 
  clone channels. This way you only need to enter this basic information once.
</para>

<para>
  At the end of <xref linkend="introTimeSlot"/>, I mentioned that trans-regional communication is 
  happening on time slot 1 while regional communication is happening on time slot 2. This is 
  visible in this example. The repeater is located in the region Berlin/Brandenbug (Ber/Bra),
  consequently all channels with within-region talk-groups have the time slot 2, all others have
  the time slot 1.
</para>

<para>
  The first channel <quote>DB0LDS TS1</quote> is a generic channel for the time slot 1. There is no
  default transmit contact defined for this channel. This channel can be used to perform arbitrary 
  direct and group calls by selecting a contact or talk group from the contact list. This means, 
  that a call cannot be started by simply pressing PTT on that channel. First, a contact must be 
  selected that should get called.
</para>

<para>
  The second channel <quote>DB0LDA DL TS1</quote> is almost identical to the first except for the 
  default transmit contact. Here <quote>Germany</quote> (TG262) is selected. This means, if this 
  channel is selected and the PTT is pressed, the talk group 262 is called. By configuring a 
  separate channel for this talk group allows to start a call to it without having to search for 
  it in the contact list. This also allows to temporarily subscribe this talk group on a repeater
  easily, by simply pressing PTT briefly. 
</para>

<note>
  <para>
    Irrespective of the default transmit contact, you can always answer to a call within the hang 
    time.
  </para>
</note>

<para>
  The third channel <quote>DB0LDS Sa/Th TS1</quote> is also similar to the first two. Here the 
  default transmit contact is the talk group for Saxony/Thuringia (TG2629) to be able to 
  subscribe that talk group at my local repeater and call it easily. Please not that for this 
  channel the time slot 1 is used. The repeater is located in Brandenburg and therefore any 
  communication with Saxony is inter-regional and should happen on the time slot 1. The group list
  contains only the talk group for Saxony/Thuringia and thus other inter-regional talk groups 
  are not received on that channel.
</para>

<para>
  Channels four, five and six are for repeater-local (TG9), regional (TG8) and the talk group 
  Berlin/Brandenburg (TG2621) calls. As this is all regional communication, it happens on the 
  time slot 2. Also they all have the group list <quote>Ber/Bra</quote> set (see 
  <xref linkend="tabIntroGroupLists"/>). Therefore, all regional talk groups (TG8, TG9, TG2621)
  are received on that channel. As the default transmit contact, the corresponding talk group
  is set. If the channel <quote>DB0LDS TG9 TS2</quote> is selected and the PTT is pressed, 
  a call to TG9 is repeated only by the repeater DB0LDS. If the channel <quote>DB0LDS BB 
  TS2</quote> is selected and the PTT is pressed, a call to TG2621 is repeater by almost all 
  repeaters in the region Berlin/Brandenbug. Therefore, chose a talk group that is sufficient
  for you intended communication. 
</para>

<note>
  <para>
    On any channel, you can start an arbitrary call (group, privat, all) by either selecting 
    the contact from the contact list of even simply entering the DMR number into the keypad
    of the radio. This is independent from the default contact on the current channel. In the
    end, the default transmit contact is a convenience feature. With the default contact, 
    channels for frequently used contacts can be created.
  </para>
</note>

<para>
  The so-called <glossterm>Admit Criterion</glossterm> should be set to <guilabel>Color 
  Code</guilabel> for DMR repeater channel. This means, that the radio will only transmit if the 
  channel is free and the color code of the repeater matches the color code of the channel.
</para>
</section>

<section>
<info><title>Other channel options</title></info>

<para>
  The user interface of the manufacturer CPS where you configure the channels, is usually very 
  extensiv. There is a huge amount of options that control the behavior of the channel. The 
  majority of these options are not used in ham radio applications. Some of these, however, I want
  to describe here briefly.
</para>

<para>
  The <glossterm>Admit Criterion</glossterm> was mentioned before. It controls under which 
  conditions the radios can transmit. There are usually three options. <guilabel>Always</guilabel>
  does exactly what it says: it allows to transmit always. This option should be chosen for 
  analog FM repeater channels. <guilabel>Channel free</guilabel> means that the radio will only 
  transmit if the current channel is free. This option should be choses for simplex channels.
  When <guilabel>Color code</guilabel> is selected, the radio will only transmit if the channel is
  free and the color code of the repeater matches the color code of the channel. This option should
  be chosen for DMR repeater channels.
</para>

<para>
  The <glossterm>TOT</glossterm> setting or <quote>transmit timeout</quote> secifies the maximum 
  duration of continuous transmission. After that period of continuous transmission, the radio 
  will stop the transmission automatically. The feature is used in commercial applications to avoid
  the blocking of a channel or talk group by a participant. This option has little sense in amateur 
  radio and can be set to infinity.
</para>

<para>
  The <glossterm>Emergency System</glossterm> is a method to signal an alarm or an emergency 
  situation. Also this feature is not used in amateur radio. 
</para>

<para>
  The option <glossterm>Privacy Group</glossterm> or <glossterm>Encryption Key</glossterm> refers
  to a built-in method of encrypting the traffic. This is actually forbidden in amateur radio.
</para>

<para> 
  The flags <quote>Emergency Alarm Confirmed</quote>, <quote>Private Call Confirmed</quote> and 
  <quote>Data Call Confirmed</quote> specify how the radio starts these calls. The radio will first
  establish a call to the destination and will signal once the call is <quote>confirmed</quote>. 
  Once the confirmation is received, the actual call starts. These options are not used in amateur
  radio and should be disabled as they may interfere with the normal operation.
</para>

<para>
  The option <glossterm>Talkaround</glossterm> allows to operate simplex on a repeater channel. 
  That is the radio transmits and receives on the repeater input frequency. This allows to bypass
  the repeater and to communicate directly with other participants on the same repeater channel.
  Also this option makes little sense in amateur radio.
</para>

<para>
  When the <glossterm>RX Only</glossterm> flag is enabled, the radio cannot transmit on that 
  channel. This may be useful for out-of-band monitoring channels where you are not allowed 
  to transmit.
</para>

<para>
  The <glossterm>VOX</glossterm> feature is actually used in ham radio. It stands for <quote>voice 
  operated switch</quote> and allows to start a call using the voice without the need to press PTT.
  Some radios allow to enable this option on a per-channel bases others only radio-wide.
</para>

<para>
  The <quote>Power</quote> option allows to specify the transmit power level. This can usually 
  be set in predefined steps like <guilabel>Low</guilabel>, <guilabel>Middle</guilabel>, 
  <guilabel>High</guilabel>. Some radios may also allow a fine grained setting of the power level.
</para>

<para>
  The <glossterm>Scan List</glossterm> specifies a list of channel that are scanned if a scan is
  started on that channel. This feature might be used as an alternative to a missing roaming 
  feature (see <xref linkend="introRoaming"/>). 
</para>
</section>
</section>


<section xml:id="itroCPZone">
<info><title>Assembling zones</title></info>

<para>
  Once you have assembled all channels of interest, you may notice that the list is quite long. 
  Hence all DMR radios organize the channels in so-called <glossterm>Zone</glossterm>s. Zones are 
  simple lists of channels that group them into relevant sets, usually based on the location. You 
  may therefore collect all channels for <quote>Home</quote>, <quote>Work</quote> and 
  <quote>Holidays</quote> into one zone each. How you organize your zones is up to you.
</para>

<para>
  You may also organize these channels by talk groups. This way you may implement some kind of a 
  manual roaming. Once you left the range of a repeater you may search for another one in the same
  zone. This way you stay connected to a particular talk group. In contrast to the automatic roaming,
  you have to select the repeater by hand.
</para>

<note>
  <para>
    Channels that are not assigned to any zone are usually not selectable by the radio. It is, 
    however, perfectly fine to assign a channel to several zones.
  </para>
</note>
</section>


<section xml:id="introCPScanList">
<info><title>Assembling scan lists</title></info>
<para>
  <glossterm>Scan List</glossterm>s are simple lists of channels. When the scan is started on a 
  particular channel, the channels scan list is used. The radio will then step though that list
  and may stop on a channel that shows activity. It is then possible to answer the received call.
  This function allows for observing several channels. Additionally, it is usually possible to specify
  one or more <quote>priority channels</quote> for a scan list. This channel is then visited more 
  frequently and thus monitored more intensively.
</para>
</section>
</section>