<?xml version="1.0" encoding="UTF-8"?>

<section xml:id="extAnytoneChannel"
         xmlns="http://docbook.org/ns/docbook"
         xmlns:xlink="http://www.w3.org/1999/xlink"
         xmlns:xi="http://www.w3.org/2001/XInclude">


<info>
  <title>Channel extensions</title>
</info>

<para>
  This extensions allows to set some device specific channel settings for 
  <trademark>AnyTone</trademark> devices. There are some general settings, valid for FM and DMR 
  channels as well some FM and DMR specific settings.
</para>

<example>
  <title>Examples of the <trademark>AnyTone</trademark> extensions for FM and DMR channels.</title>
  <programlisting><![CDATA[channels:
  - dmr:
    name: Example DMR channel 
    # ...
    anytone:
      talkaround: false
      frequencyCorrection: 0
      handsFree: false
      callConfirm: false
      sms: true
      smsConfirm: false
      dataACK: true
      simplexTDMA: false
      adaptiveTDMA: false
      loneWorker: false
      throughMode: false
  - fm:
    name: Example FM channel 
    # ...
    anytone:
      talkaround: false
      frequencyCorrection: 0
      handsFree: false
      reverseBurst: false
      rxCustomCTCSS: false
      txCustomCTCSS: false
      customCTCSS: 0.0
      squelchMode: Carrier
      scrambler: false
]]></programlisting>
</example>

<section>
<info>
  <title>Common channel attributes</title>
</info>

<para>
  This section describes the common channel attributes. These attributes are shared between FM
  and DMR channels.
</para>

<variablelist>
  <varlistentry>
    <term><token>talkaround</token></term>
    <listitem>
      <para>If <token>true</token>, talkaround is enabled for this channel. This will bypass the
        repeater on repeater channels and allows to talk to other participants directly.  </para>
    </listitem>
  </varlistentry>
  <varlistentry>
    <term><token>frequencyCorrection</token></term>
    <listitem>
      <para>Specifies some sort of correction to the frequency in some unknown units. Consider 
        contacting me, if you know more details about it.</para>
    </listitem>
  </varlistentry>
  <varlistentry>
    <term><token>handsFree</token></term>
    <listitem>
      <para>If <token>true</token>, the hands-free feature is enabled for this channel. The actual
        configuration of the hands-free feature happens in the general settings extension. This 
        setting is only applicable to the <productname>AT-D578UV</productname> device.</para>
    </listitem>
  </varlistentry>  
  <varlistentry>
    <term><token>fmAPRSFrequency</token></term>
    <listitem>
      <para>Optional alternative FM APRS frequency specified in the AnyTone extension to the APRS
      settings.</para>
    </listitem>
  </varlistentry>  
</variablelist>
</section>

<section>
  <info>
    <title>FM channel attributes</title>
  </info>

  <para>
    These attributes are only valid for FM channels.
  </para>

  <variablelist>
    <varlistentry>
      <term><token>reverseBurst</token></term>
      <listitem>
        <para>If <token>true</token>, a CTCSS phase-reverse burst is sent at the end of 
          transmission. This phase reversal of the CTCSS tone at the end of the transmission
          can be used to prevent a noise tail at the end of the transmission on the receiver 
          side. See 
          <ulink url="https://en.wikipedia.org/wiki/Continuous_Tone-Coded_Squelch_System#Reverse_CTCSS">Reverse CTCSS</ulink> 
          for details.</para>
      </listitem>
    </varlistentry>
    <varlistentry>
      <term><token>rxCustomCTCSS</token></term>
      <listitem>
        <para>If <token>true</token>, the custom CTCSS frequency (see <token>customCTCSS</token>) 
          is used to control the squelch.</para>
      </listitem>
    </varlistentry>
    <varlistentry>
      <term><token>txCustomCTCSS</token></term>
      <listitem>
        <para>If <token>true</token>, the custom CTCSS frequency (see <token>customCTCSS</token>) 
          is transmitted.</para>
      </listitem>
    </varlistentry>
    <varlistentry>
      <term><token>customCTCSS</token></term>
      <listitem>
        <para>Specifies a custom CTCSS frequency in Hz. The frequency can be specified with a 
          resolution of 0.1Hz.</para>
      </listitem>
    </varlistentry>
    <varlistentry>
      <term><token>squelchMode</token></term>
      <listitem>
        <para>Specifies the squelch mode. Must be one of <token>Carrier</token>, 
          <token>SubTone</token>, <token>OptSig</token>, <token>SubToneAndOptSig</token> or 
          <token>SubToneOrOptSig</token>.</para>
      </listitem>
    </varlistentry>
    <varlistentry>
      <term><token>scrambler</token></term>
      <listitem>
        <para>If <token>true</token>, the analog scrambler is enabled. It is not legal to use 
          scramblers in HAM radio.</para>
      </listitem>
    </varlistentry>
  </variablelist>
</section>  

<section>
  <info><title>DMR channel attributes</title></info>

  <para>This section describes the attributes, applicable to DMR channels on 
    <trademark>AnyTone</trademark> devices.</para>

  <variablelist>
    <varlistentry>
      <term><token>callConfirm</token></term>
      <listitem>
        <para>If <token>true</token>, the call confirmation is enabled.</para>
      </listitem>
    </varlistentry>
    <varlistentry>
      <term><token>sms</token></term>
      <listitem>
        <para>If <token>true</token>, the SMS reception is enabled.</para>
      </listitem>
    </varlistentry>
    <varlistentry>
      <term><token>smsConfirm</token></term>
      <listitem>
        <para>If <token>true</token>, the SMS confirmation is enabled.</para>
      </listitem>
    </varlistentry>
    <varlistentry>
      <term><token>dataACK</token></term>
      <listitem>
        <para>If <token>true</token>, the transmission of data acknowledgement is enabled.</para>
      </listitem>
    </varlistentry>
    <varlistentry>
      <term><token>simplexTDMA</token></term>
      <listitem>
        <para>If <token>true</token>, TDMA mode for simplex channels is enabled. This mode is also 
          known as DCDM (dual-capacity direct mode, see <xref linkend="glDCDM">DCDM</xref>)</para>
      </listitem>
    </varlistentry>
    <varlistentry>
      <term><token>adaptiveTDMA</token></term>
      <listitem>
        <para>If <token>true</token>, the adaptive TDMA mode is enabled. This makes only sense, if 
          <token>simplexTDMA</token> is enabled too. In this case, the radio is able to receive both
          simplex TDMA as well as normal simplex DMR on the channel.</para>
      </listitem>
    </varlistentry>
    <varlistentry>
      <term><token>loneWorker</token></term>
      <listitem>
        <para>If <token>true</token>, the lone-worker feature (see <xref linkend="glLoneWorker">Lone Worker</xref>) 
          is enabled for this channel. Usually not used in HAM radio.</para>
      </listitem>
    </varlistentry>
    <varlistentry>
      <term><token>throughMode</token></term>
      <listitem>
        <para>If <token>true</token>, the through mode is enabled. What ever that means. If you 
          know more about it, consider extending this section.</para>
      </listitem>
    </varlistentry>
  </variablelist>
</section>

</section>
