<?xml version="1.0" encoding="UTF-8"?>

<section xml:id="extAnytoneSettings"
         xmlns="http://docbook.org/ns/docbook"
         xmlns:xlink="http://www.w3.org/1999/xlink"
         xmlns:xi="http://www.w3.org/2001/XInclude">


<info>
  <title>Settings extension</title>
</info>

<para>
  This extensions allows to specify some device specific settings for
   <trademark>AnyTone</trademark> devices. As there are a myriad of settings for these devices, the
   settings extension is split into several sub-extensions, grouping the settings by domain.
</para>

<para>
  The <trademark>AnyTone</trademark> settings extension is a mapping named <token>anytone</token>. 
  It contains the device specific settings for AnyTone devices.
</para>

<section>
<info>
  <title>General settings attributes</title>
</info>

<variablelist>
  <title>General settings extension fields</title>
  <varlistentry>
    <term><token>subChannel</token></term>
    <listitem>
      <para>
        If <token>true</token>, the sub-channel is enabled.
      </para>
    </listitem>
  </varlistentry>
  <varlistentry>
    <term><token>selectedVFO</token></term>
    <listitem>
      <para>
        Specifies the currently selected VFO. Must be one of <token>A</token> or <token>B</token>,
        selecting VFO A and B, respectively.
      </para>
    </listitem>
  </varlistentry>
  <varlistentry>
    <term><token>modeA</token>, <token>modeB</token></term>
    <listitem>
      <para>
        Specifies the VFO mode for VFOs A and B. Must be one of <token>Memory</token> or 
        <token>VFO</token>. The former selects the memory/channel mode while the latter selects the 
        VFO mode.
      </para>
    </listitem>
  </varlistentry>
  <varlistentry>
    <term><token>zoneA</token>, <token>zoneB</token></term>
    <listitem>
      <para>
        Specifies the current zones for VFO A and B. Must be a reference to a zone.
      </para>
    </listitem>
  </varlistentry>
  <varlistentry>
    <term><token>vfoScanType</token></term>
    <listitem>
      <para>
        Specifies scan-type for the VFO mode. Must be one of <token>Time</token>,
        <token>Carrier</token> or <token>Stop</token>. Default is <token>Time</token>. If 
        <token>Time</token> is selected, the scan is stops for a specified period. If 
        <token>Carrier</token> is selected, the scan stops as long as a carrier is detected. If 
        <token>Stop</token> is selected, the scan stops entirely.
      </para>
    </listitem>
  </varlistentry>
  <varlistentry>
    <term><token>minVFOScanFrequencyVHF</token>, <token>maxVFOScanFrequencyVHF</token>, 
      <token>minVFOScanFrequencyUHF</token>, <token>maxVFOScanFrequencyUHF</token></term>
    <listitem>
      <para>
        Specifies the frequency ranges for the VFO scan in the VHF and UHF bands. These frequency 
        can be specified arbitrarily. If a unit-less floating point value is given, it is 
        interpreted as in MHz. If a unit-less integer value is given, it is interpreted as in Hz.
      </para>
    </listitem>
  </varlistentry>
  <varlistentry>
    <term><token>keepLastCaller</token></term>
    <listitem>
      <para>
        If <token>true</token>, the last caller ID is kept even, when the channel is changed. 
        Seriously, who needs that option? Just keep it or don't. Why is it so important? AnyTone
        codeplugs are full of these unnecessary settings.
      </para>
    </listitem>
  </varlistentry>
  <varlistentry>
    <term><token>vfoStep</token></term>
    <listitem>
      <para>
        Specifies the VFO tuning step-size.
      </para>
    </listitem>
  </varlistentry>
  <varlistentry>
    <term><token>steType</token>, <token>steFrequency</token>, <token>steDuration</token></term>
    <listitem>
      <para>
        Specifies the squelch-tail elimination type, frequency and duration. The type must be one of 
        <token>Off</token>, <token>Silent</token>, <token>Deg120</token>, <token>Deg180</token> or 
        <token>Deg240</token>. The frequency is specified as a floating point number in Hz. The 
        duration is specified in ms.
      </para>
      <para>
        This option is applicable to <productname>AT-D878UV</productname>, 
        <productname>AT-D878UV II</productname>, <productname>AT-D578UV</productname> and 
        <productname>DMR-6X2UV</productname> devices.
      </para>
    </listitem>
  </varlistentry>
  <varlistentry>
    <term><token>tbstFrequency</token></term>
    <listitem>
      <para>
        Specifies TBST/pilot-tone frequency used to enable/open a repeater. This should be one of 
        the common frequencies like 1000, 1450, 1750 and 2100 Hz.
      </para>
      <para>
        This option is applicable to <productname>AT-D878UV</productname>, 
        <productname>AT-D878UV II</productname>, <productname>AT-D578UV</productname> and 
        <productname>DMR-6X2UV</productname> devices.
      </para>
    </listitem>
  </varlistentry>
  <varlistentry>
    <term><token>proMode</token></term>
    <listitem>
      <para>
        If <token>true</token>, enables the professional mode. If enabled, some menu options are 
        hidden. 
      </para>
      <para>
        This option is applicable to <productname>AT-D878UV</productname>, 
        <productname>AT-D878UV II</productname> and 
        <productname>DMR-6X2UV</productname> devices.
      </para>
    </listitem>
  </varlistentry>
  <varlistentry>
    <term><token>maintainCallChannel</token></term>
    <listitem>
      <para>
        If <token>true</token>, maintains the call-channel. Whatever that now means. If you find it
        out, let it me know. 
      </para>
      <para>
        This option is applicable to <productname>AT-D878UV</productname>, 
        <productname>AT-D878UV II</productname> and 
        <productname>DMR-6X2UV</productname> devices.
      </para>
    </listitem>
  </varlistentry>
  <varlistentry>
    <term><token>bootSettings</token>, <token>powerSaveSettings</token>, <token>keySettings</token>, 
      <token>toneSettings</token>, <token>displaySettings</token>, <token>audioSettings</token>, 
      <token>menuSettings</token>, <token>autoRepeaterSettings</token>, <token>dmrSettings</token>, 
      <token>roamingSettings</token>, <token>gpsSettings</token>, 
      <token>simplexRepeaterSettings</token></term>
    <listitem>
      <para>
        Many more funny settings, grouped by domain. For details, see the descriptions below.
      </para>
    </listitem>
  </varlistentry>
</variablelist>
</section>

<section>
<info><title>Boot settings</title></info>
<para>
  Collects some settings, that control the startup of the radio. These settings are collected 
  under the <token>bootSettings</token> key within the <token>anytoneSettings</token> entry.
</para>

<variablelist>
  <title>Boot settings extension fields</title>
  <varlistentry>
    <term><token>bootDisplay</token></term>
    <listitem>
      <para>
        Specifies what is seen on the display during boot. Must be one of <token>Default</token>, 
        <token>CustomText</token> or <token>CustomImage</token>.
      </para>
    </listitem>
  </varlistentry>
  <varlistentry>
    <term><token>bootPasswordEnabled</token>, <token>bootPassword</token></term>
    <listitem>
      <para>
        Enables/disables and specifies the boot password. The boot password is a string of up to 8 
        number chars.
      </para>
    </listitem>
  </varlistentry>
  <varlistentry>
    <term><token>defaultChannel</token>, <token>zoneA</token>, <token>channelA</token>, 
      <token>zoneB</token>, <token>channelB</token></term>
    <listitem>
      <para>
        If <token>true</token>, <token>defaultChannel</token> enables the specified zones and 
        channels to be set on startup. <token>zoneA</token> and <token>zoneB</token> specify the 
        startup zone for VFOs A and B, respectively, and must reference a defined zone. While
        <token>channelA</token> and <token>channelB</token> specify the startup channels for each
        VFO. If no channels are defined, the VFO is chosen.
      </para>
    </listitem>
  </varlistentry>
  <varlistentry>
    <term><token>priorityZoneA</token>, <token>priorityZoneB</token></term>
    <listitem>
      <para>
        Specifies the priority zones for each VFO. These must reference a defined zone. 
      </para>
    </listitem>
  </varlistentry>
  <varlistentry>
    <term><token>defaultRoamingZone</token></term>
    <listitem>
      <para>
        Specifies the startup roaming zone. Must refer to a defined roaming zone.
      </para>
      <para>
        This option is applicable to <productname>AT-D878UV</productname>, 
        <productname>AT-D878UV II</productname> and <productname>AT-D578UV</productname> devices.
      </para>
    </listitem>
  </varlistentry>
  <varlistentry>
    <term><token>gpsCheck</token></term>
    <listitem>
      <para>
        Enables the GPS check on boot.
      </para>
      <para>
        This option is applicable to <productname>AT-D878UV</productname> and 
        <productname>AT-D878UV II</productname> devices.
      </para>
    </listitem>
  </varlistentry>
  <varlistentry>
    <term><token>reset</token></term>
    <listitem>
      <para>
        Enables a MCU reset on boot.
      </para>
      <para>
        This option is applicable to <productname>AT-D878UV</productname> and
        <productname>AT-D878UV II</productname> devices.
      </para>
    </listitem>
  </varlistentry>
</variablelist>
</section>

<section>
<info><title>Power-save settings</title></info>
<para>
  Collects some settings, that configure the power-save features. These settings are collected under
  the <token>powerSaveSettings</token> key within the <token>anytoneSettings</token> entry.
</para>

<variablelist>
  <title>Power-save setting extension fields</title>
  <varlistentry>
    <term><token>autoShutdown</token></term>
    <listitem>
      <para> Specifies the time-out for the automatic shut down. If <token>0</token>, the automatic 
      shut-down is disabled. </para>
    </listitem>
  </varlistentry>
  <varlistentry>
    <term><token>resetAutoShutdownOnCall</token></term>
    <listitem>
      <para>If <token>true</token>, the automatic showdown timer is reset on every call.</para>
    </listitem>
  </varlistentry>
  <varlistentry>
    <term><token>powerSave</token></term>
    <listitem>
      <para>Specifies the power-save mode. Must be one of <token>Off</token>, <token>Save50</token>
      or <token>Save66</token>. The latter two will save 50% or 66%, respectively.</para>
    </listitem>
  </varlistentry>
  <varlistentry>
    <term><token>atpc</token></term>
    <listitem>
      <para>Enables the ATPC (Adaptive Transmission Power Control). It reduces the transmission 
      power, if a strong signal is received.</para>
    </listitem>
  </varlistentry>
</variablelist>
</section>

<section>
<info><title>Keypad settings</title></info>
<para>
  Collects some settings, that configure the keypad, lock etc. These settings are collected 
  under the <token>keySettings</token> key within the <token>anytoneSettings</token> entry.
</para>
<para>
  This extension also allows to assign specific functions to the programmable function keys on the 
  radio. These are the side-keys, top-key and the front buttons labeled <keycap>P1</keycap> and 
  <keycap>P2</keycap>. The following list shows all functions, that can be assigned to each of these 
  buttons. Some function are not available on all devices.
</para>

<variablelist>
  <title>Key functions</title>
  <varlistentry>
    <term><token>Off</token></term>
    <listitem><para>No function at all.</para></listitem>
  </varlistentry>
  <varlistentry>
    <term><token>Voltage</token></term>
    <listitem><para>Shows the battery voltage. Applicable to 
      <productname>AT-D868UV</productname>, <productname>AT-D878UV</productname>, 
      <productname>AT-D878UV II</productname>, <productname>AT-D578UV</productname> and 
      <productname>DMR-6X2UV</productname>.</para></listitem>
  </varlistentry>
  <varlistentry>
    <term><token>Power</token></term>
    <listitem><para>Toggles though the power settings. Applicable to 
      <productname>AT-D868UV</productname>, <productname>AT-D878UV</productname>, 
      <productname>AT-D878UV II</productname>, <productname>AT-D578UV</productname> and 
      <productname>DMR-6X2UV</productname>.</para></listitem>
  </varlistentry>
  <varlistentry>
    <term><token>Repeater</token></term>
    <listitem><para>Toggles the talk-around feature. Applicable to 
      <productname>AT-D868UV</productname>, <productname>AT-D878UV</productname>, 
      <productname>AT-D878UV II</productname>, <productname>AT-D578UV</productname> and 
      <productname>DMR-6X2UV</productname>.</para></listitem>
  </varlistentry>
  <varlistentry>
    <term><token>Reverse</token></term>
    <listitem><para>Swaps the RX and TX frequencies. Applicable to 
      <productname>AT-D868UV</productname>, <productname>AT-D878UV</productname>, 
      <productname>AT-D878UV II</productname>, <productname>AT-D578UV</productname> and 
      <productname>DMR-6X2UV</productname>.</para></listitem>
  </varlistentry>
  <varlistentry>
    <term><token>Encryption</token></term>
    <listitem><para>Shows the encryption key selection. Applicable to 
      <productname>AT-D868UV</productname>, <productname>AT-D878UV</productname>, 
      <productname>AT-D878UV II</productname>, <productname>AT-D578UV</productname> and 
      <productname>DMR-6X2UV</productname>.</para>
    </listitem>
  </varlistentry>
  <varlistentry>
    <term><token>Call</token></term>
    <listitem><para>Performs an FM call with the configured DMTF/two-tone/five-tone ID. Applicable 
      to <productname>AT-D868UV</productname>, <productname>AT-D878UV</productname>, 
      <productname>AT-D878UV II</productname>, <productname>AT-D578UV</productname> and 
      <productname>DMR-6X2UV</productname>.</para></listitem>
  </varlistentry>
  <varlistentry>
    <term><token>VOX</token></term>
    <listitem><para>Shows the VOX level selection. Applicable to 
      <productname>AT-D868UV</productname>, <productname>AT-D878UV</productname>, 
      <productname>AT-D878UV II</productname> and <productname>DMR-6X2UV</productname>.</para>
    </listitem>
  </varlistentry>
  <varlistentry>
    <term><token>ToggleVFO</token></term>
    <listitem><para>Toggles between VFO and memory/channel mode. Applicable to 
      <productname>AT-D868UV</productname>, <productname>AT-D878UV</productname>, 
      <productname>AT-D878UV II</productname>, <productname>AT-D578UV</productname>.</para>
    </listitem>
  </varlistentry>
  <varlistentry>
    <term><token>SubPTT</token></term>
    <listitem><para>PTT for the sub channel. Only applicable for <keycap>PF1</keycap>, 
      <keycap>PF2</keycap> and <keycap>PF3</keycap> keys. Applicable to 
      <productname>AT-D868UV</productname>, <productname>AT-D878UV</productname>, 
      <productname>AT-D878UV II</productname> and <productname>DMR-6X2UV</productname>.</para>
    </listitem>
  </varlistentry>
  <varlistentry>
    <term><token>Scan</token></term>
    <listitem><para>Starts/stops a scan. Applicable to 
      <productname>AT-D868UV</productname>, <productname>AT-D878UV</productname>, 
      <productname>AT-D878UV II</productname>, <productname>AT-D578UV</productname> and 
      <productname>DMR-6X2UV</productname>.</para></listitem>
  </varlistentry>
  <varlistentry>
    <term><token>WFM</token></term>
    <listitem><para>Toggles the WFM (or Air band) receiver. Applicable to 
      <productname>AT-D868UV</productname>, <productname>AT-D878UV</productname>, 
      <productname>AT-D878UV II</productname>, <productname>AT-D578UV</productname> and 
      <productname>DMR-6X2UV</productname>.</para></listitem>
  </varlistentry>
  <varlistentry>
    <term><token>Alarm</token></term>
    <listitem><para>Starts/stops an alarm call. Applicable to 
      <productname>AT-D878UV</productname>, <productname>AT-D878UV II</productname>, 
      <productname>AT-D578UV</productname> and 
      <productname>DMR-6X2UV</productname>.</para></listitem>
  </varlistentry>
  <varlistentry>
    <term><token>RecordSwitch</token></term>
    <listitem><para>Enables/disables recoding function. Applicable to 
      <productname>AT-D868UV</productname>, <productname>AT-D878UV</productname>, 
      <productname>AT-D878UV II</productname>, <productname>AT-D578UV</productname> and 
      <productname>DMR-6X2UV</productname>.</para></listitem>
  </varlistentry>
  <varlistentry>
    <term><token>Record</token></term>
    <listitem><para>Start/stops a recoding. Applicable to 
      <productname>AT-D868UV</productname>, <productname>AT-D878UV</productname>, 
      <productname>AT-D878UV II</productname>, <productname>AT-D578UV</productname> and 
      <productname>DMR-6X2UV</productname>.</para></listitem>
  </varlistentry>
  <varlistentry>
    <term><token>SMS</token></term>
    <listitem><para>Start writing an SMS. Applicable to 
      <productname>AT-D868UV</productname>, <productname>AT-D878UV</productname>, 
      <productname>AT-D878UV II</productname>, <productname>AT-D578UV</productname> and 
      <productname>DMR-6X2UV</productname>.</para></listitem>
  </varlistentry>
  <varlistentry>
    <term><token>Dial</token></term>
    <listitem><para>Start manual dial. Applicable to 
      <productname>AT-D868UV</productname>, <productname>AT-D878UV</productname>, 
      <productname>AT-D878UV II</productname>, <productname>AT-D578UV</productname> and 
      <productname>DMR-6X2UV</productname>.</para></listitem>
  </varlistentry>
  <varlistentry>
    <term><token>GPSInformation</token></term>
    <listitem><para>Applicable to <productname>AT-D868UV</productname>, 
      <productname>AT-D578UV</productname> and 
      <productname>DMR-6X2UV</productname>.</para> </listitem>
  </varlistentry>
  <varlistentry>
    <term><token>Monitor</token></term>
    <listitem><para>Enables the (FM) monitor. Applicable to 
      <productname>AT-D868UV</productname>, <productname>AT-D878UV</productname>, 
      <productname>AT-D878UV II</productname>, <productname>AT-D578UV</productname> and 
      <productname>DMR-6X2UV</productname>.</para></listitem>
  </varlistentry>
  <varlistentry>
    <term><token>ToggleMainChannel</token></term>
    <listitem><para>Toggles between VFOs A and B for the main channel. Applicable to 
      <productname>AT-D868UV</productname>, <productname>AT-D878UV</productname>, 
      <productname>AT-D878UV II</productname>, <productname>AT-D578UV</productname> and 
      <productname>DMR-6X2UV</productname>.</para></listitem>
  </varlistentry>
  <varlistentry>
    <term><token>HotKey1</token>, <token>HotKey2</token>, <token>HotKey3</token>, 
      <token>HotKey4</token>, <token>HotKey5</token>, <token>HotKey6</token></term>
    <listitem><para>Triggers one of the programmed hot-key function. Applicable to 
      <productname>AT-D868UV</productname>, <productname>AT-D878UV</productname>, 
      <productname>AT-D878UV II</productname>, <productname>AT-D578UV</productname> and 
      <productname>DMR-6X2UV</productname>.</para></listitem>
  </varlistentry>
  <varlistentry>
    <term><token>WorkAlone</token></term>
    <listitem><para>Toggles the lone-worker mode. Applicable to 
      <productname>AT-D868UV</productname>, <productname>AT-D878UV</productname>, 
      <productname>AT-D878UV II</productname>, <productname>AT-D578UV</productname> and 
      <productname>DMR-6X2UV</productname>.</para></listitem>
  </varlistentry>
  <varlistentry>
    <term><token>SkipChannel</token></term>
    <listitem><para>During a scan, use this function to skip the current channel. Applicable to 
      <productname>AT-D868UV</productname>, <productname>AT-D878UV</productname>, 
      <productname>AT-D878UV II</productname>, <productname>AT-D578UV</productname> and 
      <productname>DMR-6X2UV</productname>.</para></listitem>
  </varlistentry>
  <varlistentry>
    <term><token>DigitalMonitor</token></term>
    <listitem><para>Toggles the digital monitor. Applicable to 
      <productname>AT-D868UV</productname>, <productname>AT-D878UV</productname>, 
      <productname>AT-D878UV II</productname>, <productname>AT-D578UV</productname> and 
      <productname>DMR-6X2UV</productname>.</para></listitem>
  </varlistentry>
  <varlistentry>
    <term><token>SubChannel</token></term>
    <listitem><para>Enables/disables the sub-channel. Applicable to 
      <productname>AT-D868UV</productname>, <productname>AT-D878UV</productname>, 
      <productname>AT-D878UV II</productname>, <productname>AT-D578UV</productname> and 
      <productname>DMR-6X2UV</productname>.</para></listitem>
  </varlistentry>
  <varlistentry>
    <term><token>PriorityZone</token></term>
    <listitem><para>Change to the priority zone. Applicable to 
      <productname>AT-D868UV</productname>, <productname>AT-D878UV</productname>, 
      <productname>AT-D878UV II</productname>, <productname>AT-D578UV</productname> and 
      <productname>DMR-6X2UV</productname>.</para></listitem>
  </varlistentry>
  <varlistentry>
    <term><token>VFOScan</token></term>
    <listitem><para>Toggles the VFO scan. Applicable to <productname>AT-D868UV</productname>, 
      <productname>AT-D878UV</productname>, <productname>AT-D878UV II</productname>, 
      <productname>AT-D578UV</productname> and <productname>DMR-6X2UV</productname>.</para>
    </listitem>
  </varlistentry>
  <varlistentry>
    <term><token>MICSoundQuality</token></term>
    <listitem><para>Toggle <quote>enhanced</quote> sound mode in DMR mode. Applicable to 
      <productname>AT-D868UV</productname>, <productname>AT-D878UV</productname>, 
      <productname>AT-D878UV II</productname>, <productname>AT-D578UV</productname> and 
      <productname>DMR-6X2UV</productname>.</para></listitem>
  </varlistentry>
  <varlistentry>
    <term><token>LastCallReply</token></term>
    <listitem><para>Allows to answer the last call, after the hang-time has passed. Applicable to 
      <productname>AT-D868UVE</productname>, <productname>AT-D878UV</productname>, 
      <productname>AT-D578UV</productname> and <productname>DMR-6X2UV</productname>.</para>
    </listitem>
  </varlistentry>
  <varlistentry>
    <term><token>ChannelType</token></term>
    <listitem><para>Change the channel type. Applicable to <productname>AT-D868UV</productname>, 
      <productname>AT-D878UV</productname>, <productname>AT-D878UV II</productname>, 
      <productname>AT-D578UV</productname> and <productname>DMR-6X2UV</productname>.</para>
    </listitem>
  </varlistentry>
  <varlistentry>
    <term><token>SimplexRepeater</token></term>
    <listitem><para>Enables/disables the simplex repeater feature. Applicable to 
      <productname>DMR-6X2UV</productname>.</para>
    </listitem>
  </varlistentry>
  <varlistentry>
    <term><token>Ranging</token></term>
    <listitem><para>Applicable to <productname>AT-D868UV</productname>, 
      <productname>AT-D578UV</productname> and 
      <productname>DMR-6X2UV</productname> </para></listitem>
  </varlistentry>
  <varlistentry>
    <term><token>Roaming</token></term>
    <listitem><para>Manually starts roaming. Applicable to <productname>AT-D878UV</productname>, 
      <productname>AT-D878UV II</productname>, <productname>AT-D578UV</productname> and 
      <productname>DMR-6X2UV</productname>. </para></listitem>
  </varlistentry>
  <varlistentry>
    <term><token>ChannelRanging</token></term>
    <listitem><para>Applicable to <productname>AT-D868UV</productname>, 
      <productname>AT-D578UV</productname> and 
      <productname>DMR-6X2UV</productname> </para></listitem>
  </varlistentry>
  <varlistentry>
    <term><token>MaxVolume</token></term>
    <listitem><para>Shows the maximum volume setting. Applicable to 
      <productname>AT-D868UV</productname>, <productname>AT-D878UV</productname>, 
      <productname>AT-D878UV II</productname>, <productname>AT-D578UV</productname> and 
      <productname>DMR-6X2UV</productname>.</para></listitem>
  </varlistentry>
  <varlistentry>
    <term><token>Slot</token></term>
    <listitem><para>Changes the time-slot, <productname>AT-D868UV</productname>, 
      <productname>AT-D878UV II</productname>, <productname>AT-D578UV</productname> and 
      <productname>DMR-6X2UV</productname>.</para></listitem>
  </varlistentry>
  <varlistentry>
    <term><token>Squelch</token></term>
    <listitem><para>Shows squelch settings. Applicable to 
      <productname>AT-D578UV</productname> and <productname>DMR-6X2UV</productname>.</para>
    </listitem>
  </varlistentry>
  <varlistentry>
    <term><token>APRSTypeSwitch</token></term>
    <listitem><para>Applicable to <productname>AT-D578UV</productname>.</para></listitem>
  </varlistentry>
  <varlistentry>
    <term><token>Zone</token></term>
    <listitem><para>Shows the zone selection dialog. Applicable to 
      <productname>AT-D878UV</productname>, <productname>AT-D878UV II</productname>, 
      <productname>AT-D578UV</productname> and 
      <productname>DMR-6X2UV</productname>.</para></listitem>
  </varlistentry>
  <varlistentry>
    <term><token>RoamingSet</token></term>
    <listitem><para>Shows the roaming settings(?). Applicable to 
      <productname>AT-D878UV</productname>, <productname>AT-D878UV II</productname> and 
      <productname>DMR-6X2UV</productname>.</para></listitem>
  </varlistentry>
  <varlistentry>
    <term><token>APRSSet</token></term>
    <listitem><para>???</para></listitem>
  </varlistentry>
  <varlistentry>
    <term><token>Mute</token></term>
    <listitem><para>Mutes the radio for a specified interval. Applicable to 
      <productname>AT-D878UV</productname>, <productname>AT-D878UV II</productname> and 
      <productname>DMR-6X2UV</productname>.</para></listitem>
  </varlistentry>
  <varlistentry>
    <term><token>MuteA</token>, <token>MuteB</token></term>
    <listitem><para>Mutes the VFO A/B for a specified interval. Applicable to 
      <productname>AT-D578UV</productname>.</para></listitem>
  </varlistentry>
  <varlistentry>
    <term><token>XBandRepeater</token></term>
    <listitem><para>Enables the cross-band repeater function. Applicable to 
      <productname>AT-D578UV</productname>.</para></listitem>
  </varlistentry>
  <varlistentry>
    <term><token>Speaker</token></term>
    <listitem><para>Applicable to <productname>AT-D578UV</productname>.</para>
    </listitem>
  </varlistentry>
  <varlistentry>
    <term><token>CtcssDcsSet</token></term>
    <listitem><para>Shows the CTCSS/DCS settings for FM channels. Applicable to 
      <productname>AT-D878UV</productname>, <productname>AT-D878UV II</productname> and 
      <productname>DMR-6X2UV</productname>.</para></listitem>
  </varlistentry>
  <varlistentry>
    <term><token>TBSTSend</token></term>
    <listitem><para>Sends the TBST tone. Applicable to <productname>AT-D878UV</productname>, 
      <productname>AT-D878UV II</productname>, <productname>AT-D578UV</productname>. </para>
    </listitem>
  </varlistentry>
  <varlistentry>
    <term><token>Bluetooth</token></term>
    <listitem><para>Enables/disables bluetooth function. Applicable to 
      <productname>AT-D878UV</productname>, <productname>AT-D878UV II</productname>,
      <productname>AT-D578UV</productname>.</para></listitem>
  </varlistentry>
  <varlistentry>
    <term><token>GPS</token></term>
    <listitem><para>Enables/disables GPS. Applicable to <productname>AT-D878UV</productname>, 
      <productname>AT-D878UV II</productname>, <productname>AT-D578UV</productname>.</para></listitem>
  </varlistentry>
  <varlistentry>
    <term><token>ChannelName</token></term>
    <listitem><para>Toggle channel name and frequency display. Applicable to 
      <productname>AT-D878UV</productname>, <productname>AT-D878UV II</productname>,
      <productname>AT-D578UV</productname>.</para></listitem>
  </varlistentry>
  <varlistentry>
    <term><token>CDTScan</token></term>
    <listitem><para>Starts CTCSS/DCS scan for FM channel. Applicable to 
      <productname>AT-D878UV</productname>, <productname>AT-D878UV II</productname>, 
      <productname>AT-D578UV</productname>.</para></listitem>
  </varlistentry>
  <varlistentry>
    <term><token>APRSSend</token></term>
    <listitem><para>Transmits the positioning information. Applicable to 
      <productname>AT-D878UV</productname>, <productname>AT-D878UV II</productname>,
      <productname>AT-D578UV</productname> and 
      <productname>DMR-6X2UV</productname>.</para></listitem>
  </varlistentry>
  <varlistentry>
    <term><token>APRSInfo</token></term>
    <listitem><para>Shows received APRS information. Applicable to 
      <productname>AT-D878UV</productname>, <productname>AT-D878UV II</productname>,
      <productname>AT-D578UV</productname> and 
      <productname>DMR-6X2UV</productname>.</para></listitem>
  </varlistentry>
  <varlistentry>
    <term><token>GPSRoaming</token></term>
    <listitem><para>Applicable to <productname>AT-D578UV</productname>.</para></listitem>
  </varlistentry>
  <varlistentry>
    <term><token>NoiseReductionTX</token></term>
    <listitem><para>Applicable to <productname>AT-D578UV</productname>.</para></listitem>
  </varlistentry>
</variablelist>

<para>
  The following list contains all keypad setting fields.
</para>

<variablelist>
  <title>Keypad settings extension fields</title>
  <varlistentry>
    <term><token>funcKey1Short</token>, <token>funcKey1Long</token>, <token>funcKey2Short</token>, 
      <token>funcKey2Long</token>, <token>funcKey3Short</token>, <token>funcKey3Long</token>, 
      <token>funcKey4Short</token>, <token>funcKey4Long</token>, <token>funcKey5Short</token>, 
      <token>funcKey5Long</token>, <token>funcKey6Short</token>, <token>funcKey6Long</token></term>
    <listitem>
      <para>
        Specifies the functions associated with the function keys <keycap>P1</keycap>-<keycap>P6</keycap>
        for a short and long press. Must be one of the items in the key function list above. The 
        function keys 1-6 are labeled <keycap>P1</keycap>-<keycap>P6</keycap> and are located either 
        below or next to the display.
      </para>
    </listitem>
  </varlistentry>
  <varlistentry>
    <term><token>funcKeyAShort</token>, <token>funcKeyALong</token></term>
    <listitem>
      <para>
        Specifies the function associated with the programmable function key <keycap>PF1</keycap> or 
        <keycap>A</keycap>. This button is located right below the PTT button (on handheld radios) 
        or labeled <keycap>A</keycap> on the hand microphone (<productname>AT-D578UV</productname>).
      </para>
    </listitem>
  </varlistentry>
    <varlistentry>
    <term><token>funcKeyBShort</token>, <token>funcKeyBLong</token></term>
    <listitem>
      <para>
        Specifies the function associated with the programmable function key <keycap>PF2</keycap> or 
        <keycap>B</keycap>. This button is the second one below the PTT button (on handheld radios) 
        or labeled <keycap>B</keycap> on the hand microphone (<productname>AT-D578UV</productname>).
      </para>
    </listitem>
  </varlistentry>
  <varlistentry>
    <term><token>funcKeyCShort</token>, <token>funcKeyCLong</token></term>
    <listitem>
      <para>
        Specifies the function associated with the programmable function key <keycap>PF3</keycap> or 
        <keycap>C</keycap>. THis button is the colorful one on the top (on handheld radios) or 
        labeled <keycap>C</keycap> on the hand microphone (<productname>AT-D578UV</productname>).
      </para>
    </listitem>
  </varlistentry>
  <varlistentry>
    <term><token>funcKeyDShort</token>, <token>funcKeyDLong</token></term>
    <listitem>
      <para>
        Specifies the function associated with the programmable function key <keycap>D</keycap>. 
        This button is located on the hand microphone (<productname>AT-D578UV</productname> only).
      </para>
    </listitem>
  </varlistentry>
  <varlistentry>
    <term><token>longPressDuration</token></term>
    <listitem>
      <para>
        Specifies the minimum duration of a <quote>long press</quote> on one of the programmable 
        function keys. 
      </para>
    </listitem>
  </varlistentry>
  <varlistentry>
    <term><token>autoKeyLock</token></term>
    <listitem>
      <para>
        Enables/disables the automatic key lock.
      </para>
    </listitem>
  </varlistentry>
  <varlistentry>
    <term><token>knobLock</token>, <token>keypadLock</token>, <token>sideKeysLock</token></term>
    <listitem>
      <para>
        Specifies, whether the knob, keypad and side-keys are locked, when the key-lock is enabled.
      </para>
    </listitem>
  </varlistentry>
  <varlistentry>
    <term><token>forcedKeyLock</token></term>
    <listitem>
      <para>
        Don't use. Prevents the manual key-lock release. Only applicable to commercial applications.
      </para>
    </listitem>
  </varlistentry>
</variablelist>
</section>

<section>
<info><title>Tone settings</title></info>
<para>
  Collects some settings, that configure signal tones. These settings are collected 
  under the <token>toneSettings</token> key within the <token>anytoneSettings</token> entry.
</para>

<variablelist>
  <title>Tone settings extension fields</title>
  <varlistentry>
    <term><token>keyTone</token></term>
    <listitem><para>Enables the key-pad tones. Should be disabled.</para></listitem>
  </varlistentry>
  <varlistentry>
    <term><token>keyToneLevel</token></term>
    <listitem><para>Specifies the key-tone level, 0 means user adjustable.</para></listitem>
  </varlistentry>
  <varlistentry>
    <term><token>smsAlert</token></term>
    <listitem><para>Enables the SMS alert tone.</para></listitem>
  </varlistentry>
  <varlistentry>
    <term><token>callAlert</token></term>
    <listitem><para>Enables the call alert tone. See also <token>callMelody</token>.</para></listitem>
  </varlistentry>
  <varlistentry>
    <term><token>dmrTalkPermit</token>, <token>fmTalkPermit</token></term>
    <listitem><para>Enables the DMR talk permit tone.</para></listitem>
  </varlistentry>
  <varlistentry>
    <term><token>dmrReset</token></term>
    <listitem><para>Enables the DMR reset tone. See also <token>resetMelody</token>.</para></listitem>
  </varlistentry>
  <varlistentry>
    <term><token>dmrIdle</token>, <token>fmIdle</token></term>
    <listitem><para>Enables the idle tone (for DMR and FM channels). See also <token>idleMelody</token>.</para></listitem>
  </varlistentry>
  <varlistentry>
    <term><token>startup</token></term>
    <listitem><para>Enables a startup tone.</para></listitem>
  </varlistentry>
  <varlistentry>
    <term><token>tot</token></term>
    <listitem><para>Transmit time-out warning tone.</para></listitem>
  </varlistentry>
  <varlistentry>
    <term><token>callMelody</token>, <token>idleMelody</token>, <token>resetMelody</token>, 
      <token>callEndMelody</token></term>
    <listitem><para>Specifies the melody played on each of these occasions. These melodies can 
    contain up to 5 notes (and pauses). For the sake of simplicity, qdmr supports the LilyPond 
    musical notation for these melodies. E.g., <code>a8 b e2 des4 d</code>. </para></listitem>
  </varlistentry>
</variablelist>
</section>

<section>
<info><title>Display settings</title></info>
<para>
  Collects all display settings. These settings are collected under the 
  <token>displaySettings</token> key within the <token>anytoneSettings</token> entry.
</para>

<variablelist>
  <title>Display settings extension fields</title>
  <varlistentry>
    <term><token>displayFrequency</token></term>
    <listitem>
      <para>If true, the channel frequency is shown instead of the channel name.</para>
    </listitem>
  </varlistentry>
  <varlistentry>
    <term><token>brightness</token></term>
    <listitem>
      <para>Specifies the brightness of the backlight in a range 1-10.</para>
    </listitem>
  </varlistentry>
  <varlistentry>
    <term><token>backlightDuration</token>, <token>backlightDurationRX</token>, 
      <token>backlightDurationTX</token></term>
    <listitem>
      <para>Specifies the backlight duration. While setting the TX backlight duration to 0 disables
      it during TX, setting the RX backlight duration to that value, enables it continously.</para>
    </listitem>
  </varlistentry>
  <varlistentry>
    <term><token>customChannelBackground</token></term>
    <listitem>
      <para>If <token>true</token>, the custom channel background is enabled.</para>
    </listitem>
  </varlistentry>
  <varlistentry>
    <term><token>volumeChangePrompt</token>, <token>callEndPrompt</token></term>
    <listitem>
      <para>If <token>true</token> the volume change and call-end prompts are shown.</para>
    </listitem>
  </varlistentry>
  <varlistentry>
    <term><token>showClock</token>, <token>showCall</token>, <token>showContact</token>,
      <token>showChannelNumber</token>, <token>showColorCode</token>, <token>showTimeSlot</token>,
      <token>showChannelType</token>, <token>showLastHeard</token></term>
    <listitem>
      <para>Enables/disables various display elements.</para>
    </listitem>
  </varlistentry>
  <varlistentry>
    <term><token>lastCallerDisplay</token></term>
    <listitem>
      <para>Specifies how the last caller is shown. Must be one of <token>Off</token>, 
      <token>ID</token>, <token>Call</token> or <token>Both</token></para>
    </listitem>
  </varlistentry>
  <varlistentry>
    <term><token>callColor</token></term>
    <listitem>
      <para>Specifies the call color. Must be one of <token>White</token>, <token>Black</token>, 
      <token>Orange</token>, <token>Red</token>, <token>Yellow</token>, <token>Green</token>, 
      <token>Turquoise</token>, <token>Blue</token>. Please note, that not all devices allow for 
      all colors. Especially the <productname>AT-D868UV</productname> has only limited colors.</para>
    </listitem>
  </varlistentry>
  <varlistentry>
    <term><token>standbyTextColor</token>, <token>standbyBackgroundColor</token></term>
    <listitem>
      <para>Specifies the text or background color in stand-by. Must be one of <token>White</token>, 
      <token>Black</token>, <token>Orange</token>, <token>Red</token>, <token>Yellow</token>, 
      <token>Green</token>, <token>Turquoise</token>, <token>Blue</token>. Please note, that not all
      devices allow for all colors. Applicable to <productname>AT-D878UV</productname>, 
      <productname>AT-D878UV II</productname>, <productname>AT-D578UV</productname> and 
      <productname>DMR-6X2UV</productname>.</para>
    </listitem>
  </varlistentry>
  <varlistentry>
    <term><token>channelNameColor</token>, <token>channelBNameColor</token></term>
    <listitem>
      <para>Specifies the color of the channel name. Must be one of <token>White</token>, 
      <token>Black</token>, <token>Orange</token>, <token>Red</token>, <token>Yellow</token>, 
      <token>Green</token>, <token>Turquoise</token>, <token>Blue</token>. Please note, that not all
      devices allow for all colors. Applicable to <productname>AT-D878UV</productname>, 
      <productname>AT-D878UV II</productname> and <productname>AT-D578UV</productname>.</para>
    </listitem>
  </varlistentry>
  <varlistentry>
    <term><token>zoneNameColor</token>, <token>zoneBNameColor</token></term>
    <listitem>
      <para>Specifies the color of the channel name. Must be one of <token>White</token>, 
      <token>Black</token>, <token>Orange</token>, <token>Red</token>, <token>Yellow</token>, 
      <token>Green</token>, <token>Turquoise</token>, <token>Blue</token>. Please note, that not all
      devices allow for all colors. Applicable to <productname>AT-D878UV</productname>, 
      <productname>AT-D878UV II</productname> and <productname>AT-D578UV</productname>.</para>
    </listitem>
  </varlistentry>
  <varlistentry>
    <term><token>language</token></term>
    <listitem>
      <para>Specifies the UI language. Must be one of <token>English</token> or 
      <token>German</token>. Applicable to <productname>AT-D878UV</productname>, 
      <productname>AT-D878UV II</productname>, <productname>AT-D578UV</productname> and 
      <productname>DMR-6X2UV</productname>.</para>
    </listitem>
  </varlistentry>
  <varlistentry>
    <term><token>dateFormat</token></term>
    <listitem>
      <para>Specifies the date format. Must be one of <token>YearFirst</token> (i.e., yyyy/mm/dd) or 
        <token>DayFirst</token> (i.e., dd/mm/yyyy). Obviously, they got everything covered.</para>
    </listitem>
  </varlistentry>
</variablelist>
</section>

<section>
<info><title>Audio settings</title></info>
<para>
  This entry collects all audio-related settings. These settings are collected under the 
  <token>audioSettings</token> key within the <token>anytoneSettings</token> entry. 
</para>

<variablelist>
<title>Audio settings extension fields</title>
<varlistentry>
  <term><token>voxDelay</token></term>
  <listitem>
    <para>An interval specifying the delay to activate the VOX. Stored in ms resolution. </para>
  </listitem>
</varlistentry>
<varlistentry>
  <term><token>voxSource</token></term>
  <listitem>
    <para>Specifies the source for the VOX. Must be one of <token>Internal</token>, 
    <token>External</token> or <token>Both</token>.</para>
  </listitem>
</varlistentry>
<varlistentry>
  <term><token>recording</token></term>
  <listitem>
    <para>If <token>true</token>, recording is enabled.</para>
  </listitem>
</varlistentry>
<varlistentry>
  <term><token>enhance</token></term>
  <listitem>
    <para>If <token>true</token>, enabled some TX audio enhancement. I don't know what it does nor 
    if it is reasonable to enable.</para>
  </listitem>
</varlistentry>
<varlistentry>
  <term><token>muteDelay</token></term>
  <listitem>
    <para>Specifies some muting delay in minutes.</para>
  </listitem>
</varlistentry>
<varlistentry>
  <term><token>maxVolume</token>, <token>maxHeadPhoneVolume</token></term>
  <listitem>
    <para>Specifies the maximum speaker and headphone volume.</para>
  </listitem>
</varlistentry>
<varlistentry>
  <term><token>enableFMMicGain</token>, <token>fmMicGain</token></term>
  <listitem>
    <para>Enables and sets a separate microphone gain for FM. If disabled, the global mic gain 
    is used for both, DMR and FM.</para>
  </listitem>
</varlistentry>
</variablelist>
</section>

<section>
<info><title>Menu settings</title></info>
<para>
    This entry collects all menu-related settings (there aren't many). These settings are collected 
    under the <token>menuSettings</token> key within the <token>anytoneSettings</token> entry. 
</para>

<variablelist>
<title>Menu settings extension fields</title>
<varlistentry>
  <term><token>duration</token></term>
  <listitem>
    <para>Specifies the duration, the menu is shown.</para>
  </listitem>
</varlistentry>
<varlistentry>
  <term><token>separator</token></term>
  <listitem>
    <para>If <token>true</token>, the menu items are separated by a line. Again WTF AnyTone? Why 
    the hack is an option needed for this? For me, this is just another useless option to check on 
    every firmware update.</para>
  </listitem>
</varlistentry>
</variablelist>
</section>

<section>
<info><title>Auto-Repeater settings</title></info>
<para>
  The auto-repeater settings of anytone-devices is quiet complex. It allows to specify rules, in 
  which frequency ranges some auto-repeater settings are applied referencing a particular offset
  for that rule. These offsets are specified within a separate list of frequency offsets. 
</para>
<para>
  These settings are needlessly complicated. It would be sufficient to specify a range and offset. 
  AnyTone, however, decided that this would be way to simple and user friendly. However, fitting 
  their concept into qdmr's concept of references to objects, makes it even worse. You will see.
</para>
<para>
  The auto-repeater settings are specified within the <token>autoRepeaterSettings</token> item
  within the <token>anytoneSettings</token> item.
</para>

<variablelist>
<title>Auto-repeater extension fields</title>
<varlistentry>
  <term><token>directionA</token>, <token>directionB</token></term>
  <listitem>
    <para>Specifies the direction of the repeater offset for VFO A and B. I have absolutely no 
    clue, why this depends on the VFO and not on the BAND (VHF/UHF) or even per offset. Only the 
    wise people at AnyTone will know the answer.</para>
    <para>However, must be one of <token>Off</token>, <token>Positive</token> or 
    <token>Negative</token>.</para>
  </listitem>
</varlistentry>
<varlistentry>
  <term><token>vhfMin</token>, <token>vhfMax</token>, <token>uhfMin</token>, <token>uhfMax</token>,
    <token>vhf2Min</token>, <token>vhf2Max</token>, <token>uhf2Min</token>, <token>uhf2Max</token></term>
  <listitem>
    <para>Specifies the VHF and UHF frequency range for which the auto-repeater feature is defined. 
    These can be any frequencies by the way.</para>
    <para>The <token>vhf2</token> and <token>uhf2</token> 
    variants are only present for <productname>AT-D878UV</productname>, 
    <productname>AT-D878UV II</productname> and <productname>AT-D578UV</productname> radios and 
    allow for a second pair of frequency ranges with a different offset.</para>
  </listitem>
</varlistentry>
<varlistentry>
  <term><token>vhf</token>, <token>uhf</token>, <token>vhf2</token>, <token>uhf2</token></term>
  <listitem>
    <para>References the offset for the VHF and UHF frequency range specified above. This must be 
    a reference to one of the auto-repeater offsets defined below. </para>
    <para>The <token>vhf2</token> and <token>uhf2</token> references are only present for 
    <productname>AT-D878UV</productname>, <productname>AT-D878UV II</productname> and 
    <productname>AT-D578UV</productname> radios and allow for a different offset.</para>
  </listitem>
</varlistentry>
<varlistentry>
  <term><token>offset</token></term>
  <listitem>
    <para>A list of auto-repeater offsets. As qdmr only allows references to named objects, they 
    must be relatively complex. Each entry has an ID (to reference the offset), name (because qdmr 
    objects have names) and the actual offset frequency. See below for a description of these 
    elements.</para>
  </listitem>
</varlistentry>
</variablelist>

<section>
<info><title>Auto-repeater offsets</title></info>
<para>
  As mentioned above, qdmr requires any object referenced within the codeplug to be a proper
  object. That is with an ID and name. This makes sense, as almost all referenced elements within 
  the codeplug are complex objects and have a display name. However, AnyTone decided to reference a 
  mere offset frequency. Consequently, you have to give names to them in qdmr. Sorry.
</para>
<para>
  The below you find a list with the properties of the offset frequencies.
</para>

<variablelist>
<title>Offset frequency fields</title>
<varlistentry>
  <term><token>id</token></term>
  <listitem>
    <para>Specifies the unique ID of the offset frequency. Used to reference it.</para>
  </listitem>
</varlistentry>
<varlistentry>
  <term><token>name</token></term>
  <listitem>
    <para>Specifies the name of the offset frequency. Any string is valid and not needed. However, 
    references are shown in qdmr with their name. So don't keep that field empty.</para>
  </listitem>
</varlistentry>
<varlistentry>
  <term><token>offset</token></term>
  <listitem>
    <para>Specifies the actual frequency offset. </para>
  </listitem>
</varlistentry>
</variablelist>
</section>

<example>
<title>An example for two auto-repeater frequency ranges active only on VFO A.</title>
 <programlisting><![CDATA[anytoneSettings:
  # ...  
  autoRepeaterSettings:
    directionA: Negative   # <- Only on VFO A. Because.
    directionB: Off
    # VHF range 
    vhfMin: 145.569 MHz
    vhfMax: 145.794 MHz
    vhf: offsetVHF
    # UHF range
    uhfMin: 438.55 MHz
    uhfMax: 439.4375 MHz
    uhf: offsetUHF
    # Some generic but disabled ranges. 
    vhf2Min: 136 MHz
    vhf2Max: 174 MHz
    vhf2: ~
    uhf2Min: 400 MHz
    uhf2Max: 480 MHz
    uhf2: ~
    # The offsets
    offset:
      - id: offsetVHF
        name: VHF
        offset: 600 kHz
      - id: offsetUHF
        name: UHF
        offset: 7.6 Mhz
  # ...  
]]></programlisting>
</example>
</section>

<section>
<info><title>DMR related settings</title></info>
<para>
  Some DMR related settings. Some of these should not be touched.
</para>

<variablelist>
<varlistentry>
  <term><token>groupCallHangTime</token>, <token>privateCallHangTime</token>, 
    <token>manualGroupCallHangTime</token>, <token>manualPrivateCallHangTime</token></term>
  <listitem>
    <para>Specifies the group and private call hang time. That is, the time, within you could answer 
    a call by pressing the PTT, even if the group or private call is not the default transmit 
    contact of the channel.</para>
  </listitem>
</varlistentry>
<varlistentry>
  <term><token>preWaveDelay</token>, <token>wakeHeadPeriod</token></term>
  <listitem>
    <para>Don't touch. Should both be 100ms.</para>
  </listitem>
</varlistentry>
<varlistentry>
  <term><token>filterOwnID</token></term>
  <listitem>
    <para>If <token>true</token>, your own ID is not shown in the call lists.</para>
  </listitem>
</varlistentry>
<varlistentry>
  <term><token>smsFormat</token></term>
  <listitem>
    <para>Specifies the SMS format. Must be one of <token>Motorola</token>, <token>Hytera</token>, 
    <token>DMR</token>.</para>
  </listitem>
</varlistentry>
<varlistentry>
  <term><token>monitorSlotMatch</token></term>
  <listitem>
    <para>Specifies if and how the DMR monitor will match the time slot of the current channel. Must
    be one of <token>Off</token>, <token>Single</token>, <token>Both</token>.</para>
  </listitem>
</varlistentry>
<varlistentry>
  <term><token>monitorColorCodeMatch</token></term>
  <listitem>
    <para>If <token>true</token>, the DMR monitor will match the color code of the current 
    channel.</para>
  </listitem>
</varlistentry>
<varlistentry>
  <term><token>monitorIDMatch</token></term>
  <listitem>
    <para>If <token>true</token>, the DMR monitor will match the DMR IDs to the group list of the 
    current channel.</para>
  </listitem>
</varlistentry>
<varlistentry>
  <term><token>monitorTimeSlotHold</token></term>
  <listitem>
    <para>If <token>true</token>, the DMR monitor will hold the time slot first received on.</para>
  </listitem>
</varlistentry>
<varlistentry>
  <term><token>sendTalkerAlias</token></term>
  <listitem>
    <para>If enabled, sends the radio name as talker alias over the air.</para>
  </listitem>
</varlistentry>
<varlistentry>
  <term><token>takerAliasSource</token></term>
  <listitem>
    <para>Specifies the source for the talker alias display. Must be one of <token>Off</token>, 
      <token>UserDB</token> or <token>Air</token>.</para>
  </listitem>
</varlistentry>
<varlistentry>
  <term><token>talkerAliasEncoding</token></term>
  <listitem>
    <para>Specifies the encoding of the taker alias. Must be one of <token>ISO8</token>,
      <token>ISO7</token> or <token>Unicode</token>. </para>
  </listitem>
</varlistentry>
</variablelist>
</section>

<section>
<info><title>GPS settings</title></info>
<para>
  This section collects settings concerning GPS position reporting. These settings are 
  collected under the <token>gpsSettings</token> key within the <token>anytoneSettings</token> entry. 
</para>

<variablelist>
<varlistentry>
  <term><token>units</token></term>
  <listitem>
    <para>Specifies the unit system to use for distance reporting (ranging). This must be one of 
    <token>Metric</token> or <token>Archaic</token>. This software was developed by a European, so 
    don't mail me to tell me, that I am silly.</para>
  </listitem>
</varlistentry>
<varlistentry>
  <term><token>timeZone</token></term>
  <listitem>
    <para>Specifies the time-zone for the device. Any IANA time-zone ID is valid here. E.g., 
    <code>Europe/Paris</code> or <code>UTC+5</code>.</para>
  </listitem>
</varlistentry>
<varlistentry>
  <term><token>reportPosition</token></term>
  <listitem>
    <para>If <token>true</token>, GPS position reporting is enabled.</para>
  </listitem>
</varlistentry>
<varlistentry>
  <term><token>updatePeriod</token></term>
  <listitem>
    <para>Specifies the update/reporting interval in seconds. Any interval specification is valid 
    here. E.g., <code>5 min</code> or <code>360 s</code>.</para>
  </listitem>
</varlistentry>
<varlistentry>
  <term><token>mode</token></term>
  <listitem>
    <para>Specifies the GPS mode. Must be one of <token>GPS</token>, <token>Beidou</token>, 
    <token>GPS_Beidou</token>, <token>Glonass</token>, <token>GPS_Glonass</token>, 
    <token>Beidou_Glonass</token> or <token>All</token>.</para>
  </listitem>
</varlistentry>
</variablelist>
</section>

<section>
<info><title>Roaming settings</title></info>
<para>
  This section collects settings concerning the roaming. These settings are collected 
  under the <token>roamingSettings</token> key within the <token>anytoneSettings</token> entry. 
</para>

<variablelist>
<varlistentry>
  <term><token>autoRoam</token></term>
  <listitem>
    <para>If <token>true</token>, the auto-roaming is enabled. If <token>false</token>, the roaming
    must be started manually.</para>
  </listitem>
</varlistentry>
<varlistentry>
  <term><token>autoRoamPeriod</token></term>
  <listitem>
    <para>Specifies the auto-roaming period in minutes. Any interval specification is valid here. 
    E.g., <code>30 min</code> or <code>1 h</code>.</para>
  </listitem>
</varlistentry>
<varlistentry>
  <term><token>autoRoamDelay</token></term>
  <listitem>
    <para>Specifies some additional delay in seconds before the auto-roaming is started. Any 
    interval specification is valid here like <code>60 s</code> or <code>1 min</code>.</para>
  </listitem>
</varlistentry>
<varlistentry>
  <term><token>roamStart</token>,<token>roamReturn</token></term>
  <listitem>
    <para>Specifies the roaming start/end condition. Must be one of <token>Periodic</token> or 
    <token>OutOfRange</token>.</para>
  </listitem>
</varlistentry>
<varlistentry>
  <term><token>rangeCheck</token></term>
  <listitem>
    <para>If <token>true</token>, the periodic range check is enabled.</para>
  </listitem>
</varlistentry>
<varlistentry>
  <term><token>checkInterval</token></term>
  <listitem>
    <para>Specifies the range check period in seconds. Any interval specification is valid here. 
    E.g., <code>3 min</code> or <code>180 s</code>. </para>
  </listitem>
</varlistentry>
<varlistentry>
  <term><token>retryCount</token></term>
  <listitem>
    <para>Number of retries to connect to a repeater before giving up and starting the roaming.</para>
  </listitem>
</varlistentry>
<varlistentry>
  <term><token>outOfRangeAlert</token></term>
  <listitem>
    <para>Specifies the alert type for the out-of-range notification. Must be one of 
    <token>Off</token>, <token>Bell</token> or <token>Voice</token></para>
  </listitem>
</varlistentry>
<varlistentry>
  <term><token>notification</token></term>
  <listitem>
    <para>If <token>true</token>, the repeater check notification is enabled.</para>
  </listitem>
</varlistentry>
<varlistentry>
  <term><token>notificationCount</token></term>
  <listitem>
    <para>The number of repeater check notifications.</para>
  </listitem>
</varlistentry>
<varlistentry>
  <term><token>defaultZone</token></term>
  <listitem>
    <para>Specifies the default roaming zone. Must be a roaming zone ID or 
    <token>null</token>.</para>
  </listitem>
</varlistentry>
<varlistentry>
  <term><token>gpsRoaming</token></term>
  <listitem>
    <para>If <token>true</token>, GPS based roaming is enabled.</para>
  </listitem>
</varlistentry>
</variablelist>
</section>

<section>
<info><title>Bluetooth settings</title></info>
<para>
  This section collects settings concerning bluetooth feature. These settings are 
  collected under the <token>bluetoothSettings</token> key within the 
  <token>anytoneSettings</token> entry. 
</para>

<variablelist>
  <varlistentry>
    <term><token>pttLatch</token></term>
    <listitem>
      <para>If <token>true</token>, the bluetooth PTT button latches.</para>
    </listitem>
  </varlistentry>
  <varlistentry>
    <term><token>pttSleepTimer</token></term>
    <listitem>
      <para>Specifies the timeout for the sleep mode of the bluetooth PTT button.</para>
    </listitem>
  </varlistentry>
</variablelist>
</section>

<section>
<info><title>Simplex repeater settings</title></info>
<para>
  Collects all settings related to the <productname>DMR-6X2UV</productname> simplex-repeater 
  feature. These settings are collected under the <token>simplexRepeaterSettings</token> key 
  within the <token>anytoneSettings</token> entry. This extension is only relevant for the 
  <productname>DMR-6X2UV</productname> series.
</para>

<variablelist>
<varlistentry>
  <term><token>enabled</token></term>
  <listitem>
    <para>If <token>true</token>, the simplex repeater function is enabled.</para>
  </listitem>
</varlistentry>
<varlistentry>
  <term><token>monitor</token></term>
  <listitem>
    <para>If <token>true</token>, the traffic can be monitored on the speaker.</para>
  </listitem>
</varlistentry>
<varlistentry>
  <term><token>timeSlot</token></term>
  <listitem>
    <para>Specifies the time-slot of the repeater. This must be one of <token>TS1</token>, 
    <token>TS2</token> or <token>Channel</token>. The latter implies, that the repeater uses the 
    time-slot of the channel.</para>
  </listitem>
</varlistentry>
</variablelist>
</section>
</section>
